
Ensure the encoder and decoder (ANT-7000E and ANT-700D) are at the same version of firmware

version: ANT-7000.v332.00

copy firmware.bin onto a fat32 formatted USB memory stick

1. power off encoder
2. plug in USB stick - adaptor is required for encoder : USB Type-A Female to USB Mini-B 5 Male Adapter
			something like https://www.amazon.co.uk/AKORD-Female-Mini-Male-Adapter/dp/B00303HSSG
3. power on encoder, the LED will flash quickly
4. Once the LED stop this fast flashing (about 5 minutes) power off cycle encoder
5. remove USB
6. power on
7. go to 192.168.0.171
8. Local S/W version Antrica.332.00(2019.04.19-17:23:41)

9. for decoder repeat steps 1 thru' 6. In step 2 no adaptor is required

10. go to 192.168.0.172
11. Local S/W version Antrica.332.00(2019.04.19-17:23:41)





